**BONAFIDE CERTIFICATE**

Certified that this project report **“CHANNEL DECODING (PORTING) FOR DRM RECEIVER”** is the bonafide work of “**M.SHARON PREETHI”** who carried out the project work under my supervision.

**SIGNATURE SIGNATURE**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Submitted for the Full Semester Viva Voce held on ……………………….

**Internal Examiner External Examiner**

**ACKNOWLEDGEMENT**

First and foremost, I praise and thank **ALMIGHTY GOD** whose blessings have bestowed in us the will power and confidence to carry out my project. I am grateful to our most respected founder (late) **Dr. D.G.S. Dhinakaran**, **C.A.I.I.B, Ph.D.,** and honourable chancellor **Dr. Paul Dhinakaran**, **M.B.A, Ph.D.,** for their grace and blessing.

I extend my thanks to our honourable vice-chancellor **Dr. S. SUNDAR MANOHARAN, Ph.D.,** and our respected registrar **Dr. C. Joseph Kennady, Ph.D.,** for the opportunity given to take up the project.

I extend my thanks to **Dr. SHOBHA REKH, M.E., Ph.D., Professor and Head of the Department of ECE** for her all time encouragement and guidance.

I convey my special thanks to my external guides **Mrs.R.Padmavathi,** Project

Manager and **Mr.Buvaneswaran**, System Engineer of **Jasmin Infotech Pvt. Ltd, Chennai-100**, for their kind encouragement and providing facilities throughout the project period.

I would like to thank the project coordinators for their support in all the project reviews. I also thank all the staff members of our department for extending their helping hands to make this project a success.

I would also like to thank all my/our friends and beloved parents who prayed and helped during the project work.

**ABSTRACT**

Radio needs to remain relevant in a digital interactive world. Digital Radio has better audio quality when compared to analog radio. DRM is a set of digital audio broadcasting technologies design to work over the frequency bands currently used for AM. It can deliver FM comparable sound quality on frequencies below 30MHz. The encoding and decoding can be performed with digital signal processing, so that a cheap embedded computer with conventional transmitter and receiver can perform the rather complex encoding and decoding.

This project gives the basic idea of channel decoding in digital radio. This process is cross compiled from Blackfin platform to Jacinto 5 platform. The project deals with the porting of the decoding process on J5 platform as it is a Multi processor and also had EDMA 3, while the previous versions of processors have EDMA 2 or EDMA 1.

**TABLE OF CONTENTS**

|  |  |  |
| --- | --- | --- |
|  | **TITLE** | **Page No.** |
|  | **BONAFIDE CERTIFICATE** | i |
|  | **ACKNOWLEDGEMENT** | ii |
|  | **ABSTRACT** | iii |
|  | **TABLE OF CONTENTS** | iv |
|  | **LIST OF FIGURES** | vii |
|  | **LIST OF TABLES** | viii |
|  | **LIST OF ABBREVIATIONS** | ix |
|  | **LIST OF SYMBOLS** | x |
| **1**. | **INTRODUCTION** | 1 |
|  | 1.2 GENERAL CHARACTERISTIC | 1 |
|  | 1.2.1 SYSTEM OVERVIEW | 2 |
|  | 1.2.2 SYSTEM ARCHITECTURE | 3 |
| **2**. | **TRANSMISSION MODES** | 5 |
|  | 2.1 SIGNAL BANDWIDTH RELATED PARAMETERS | 5 |
|  | 2.3 CODING RATES AND CONSTELLATIONS | 5 |
|  | 2.2 TRANSMISSION EFFICIENCY RELATED PARAMETERS | 5 |
|  | 2.4 OFDM PARAMETER SET | 6 |
| **3.** | **CHANNEL CODING** | 8 |
|  | 3.1 MULTIPLEX DEFINITION | 9 |
|  | 3.1.1 INTRODUCTION | 9 |
|  | 3.1.2 MAIN SERVICE CHANNEL (MSC) | 9 |
|  | 3.1.2.1 INTRODUCTION | 9 |
|  | 3.1.2.2 STRUCTURE | 9 |
|  | 3.1.2.3 BUILDING THE MSC | 10 |

|  |  |  |
| --- | --- | --- |
|  | 3.1.2.4 MULTIPLEX FRAMES | 10 |
|  | 3.1.2.5 HIERARCHICAL FRAMES | 11 |
|  | 3.1.2.6 RECONFIGURATION | 11 |
|  | 3.2 FAST ACCESS CHANNEL (FAC) | 11 |
|  | 3.2.1 INTRODUCTION | 11 |
|  | 3.2.2 STRUCTURE | 12 |
|  | 3.2.3 CHANNEL PARAMETERS | 12 |
|  | 3.2.4 SERVICE PARAMETERS | 16 |
|  | 3.3 CRC | 18 |
|  | 3.4 FAC REPETITION | 18 |
|  | 3.5 TRANSPORT MULTIPLEX ADAPTATION | 18 |
|  | 3.5.2 FAST ACCESS CHANNEL | 23 |
|  | 3.5.3 SERVICE DESCRIPTION CHANNEL | 24 |
|  | 3.6 ENERGY DISPERSAL | 24 |
| **4**. | **TAG ITEMS SPECIFYING DRM MULTIPLEX** | 27 |
|  | 4.1 ROBUSTNESS MODE (robm) | 27 |
|  | 4.2 FAST ACCESS CHANNEL (fac\_) | 28 |
|  | 4.3 SERVICE DESCRIPTION CHANNEL (sdc\_) | 28 |
|  | 4.4 MSC STREAM DATA <N> (str0, str1, str2 and str3) | 29 |
| **5.** | **DIRECT MEMORY ACCESS** | 31 |
|  | 5.1 INTERNAL DMA (IDMA): | 31 |
|  | 5.2 ENHANCED DIRECT MEMORY ACCESS (EDMA) | 31 |
|  | 5.3 EDMA3 Channel Controller (EDMA3CC) | 32 |
|  | 5.4 EDMA3 Transfer Controller (EDMA3TC) | 35 |
|  | 5.5 Types of EDMA3 Transfers | 37 |
| **6.** | **MULTICHANNEL AUDIO SERIAL PORT** | 38 |
|  | 6.1 INTRODUCTION | 38 |

|  |  |  |
| --- | --- | --- |
|  | 6.2 FEATURES | 38 |
|  | 6.3 PROTOCOLS SUPPORTED | 39 |
|  | 6.4 FORMAT | 41 |
|  | 6.4.1 TDM FORMAT | 41 |
|  | 6.4.2 INTER-INTEGRATED SOUND (I2S) FORMAT | 43 |
| **7.** | **RESULTS AND DISCUSSION** | 45 |
| **8.** | **CONCLUSION** | 55 |

**LIST OF FIGURES**

|  |  |  |
| --- | --- | --- |
| **FIGURE NO:** | **DESCRIPTION** | **Page No.** |
| 1.1 | Conceptual DRM transmission block diagram |  |
| 1.2 | DRM Receiver block diagram |  |
| 2.1 | Functional block diagram of the coding and interleaving |  |
| 3.1 | PRBS generator |  |
| 4.1 | Robustness mode |  |
| 4.2 | Fast Access Channel |  |
| 4.3 | Service Description Channel |  |
| 4.4 | MSC stream data |  |

**LIST OF TABLES**

|  |  |  |
| --- | --- | --- |
| **TABLE NO:** | **DESCRIPTION** | **PAGE NO:** |
| 1.1 | Robustness mode uses |  |
| 1.2 | OFDM symbol parameters |  |
| 3.1 | Code rate combinations for the MSC with 16-QAM(robustness modes A, B, C and D) |  |
| 3.2 | Code rate combinations for the MSC with 64-QAM(robustness modes A, B, C and D) |  |
| 3.3 | Code rate combinations for the SPP of MSC with HMsym 64-QAM(robustness modes A, B, C and D) |  |
| 3.4 | Code rate combinations for the VSPP of MSC with HMsym 64-QAM(robustness modes A, B, C and D) |  |
| 3.5 | Code rate combinations for the SPP of MSC with HMmix 64-QAM(robustness modes A, B, C and D) |  |
| 3.6 | Number of QAM cells *NSDC* for SDC |  |
| 3.7 | First 16 bits of the PRBS |  |
| 4.1 | Robustness mode encoding |  |

**LIST OF ABBREVIATIONS**

AFS - Alternative Frequency Switching

AM - Amplitude Modulation

CRC - Cyclic Redundancy Check

DRM - Digital Radio Mondiale

EEP - Equal Error Protection

FAC - Fast Access Channel

FM - Frequency Modulation

HF - High Frequency

HMmix - mixed Hierarchical Mapping

HMsym - symmetrical Hierarchical Mapping

LF - Low Frequency

MF - Medium Frequency

MSb - Most Significant bit

MSC - Main Service Channel

OFDM - Orthogonal Frequency Division Multiplexing

OIRT - Organisation Internationale de Radiodiffusion et de Télévision

Pan - Panorama

PRBS - Pseudo-Random Binary Sequence

QAM - Quadrature Amplitude Modulation

rfa - reserved for future addition

rfu - reserved for future use

SDC - Service Description Channel

SM - Standard Mapping

SPP - Standard Protected Part

UEP - Unequal Error Protection

VSPP - Very Strongly Protected Part

**LIST OF SYMBOLS**

*fR -* reference frequency of the emitted signal

*K -* number of active carriers in the OFDM symbol

*K*max *-* carrier index of the upper active carrier in the OFDM signal

*K*min *-* carrier index of the lower active carrier in the OFDM signal

*LMUX -* number of input bits per multiplex frame for the multilevel encoding

*NMUX  -* number of MSC cells (QAM symbols) per multiplex frame

*T -* elementary time period, equal to 831/3 μs (1/12 kHz)

*Tf  -* duration of the transmission frame

*Tg -* duration of the guard interval

*Ts  -* duration of an OFDM symbol

*Tsf  -* duration of the transmission super-frame built from the set of

Transmission frames

*Tu -* duration of the useful (orthogonal) part of an OFDM symbol, excluding the guard interval

*X\* -* complex conjugate of value X

*-* round towards plus infinity

*-* round towards minus infinity